Qbiss One Archicad BIM Library:
ARCHICAD family version: 11_2025   
            
1. Qbiss One Start File.pln
	Qbiss One horizontal, 
	Qbiss One vertical,
2. Favorites:
	Qbiss One Favorites.prf
3. Library:
	Qbiss_One(Q1v4).lcf
4. Schedules:
	CW-Qbiss frames-AC28.xml
	CW-Qbiss panels-AC28.xml  


HOW TO GET STARTED

01. Open Archicad 28 attached file Qbiss One Start File.pln
02. Load Qbiss One library
File -> Libraries and Objects -> Library Manager -> Add Qbiss_One(Q1v4).lcf
03. Load Qbiss One Favorites
Window -> Palettes -> Favorites -> Import/Export -> Import Qbiss One Favorites
04. Load  Qbiss One Schedules
Schedules (right click) -> Scheme Settings -> Import CW-Qbiss frames_AC28 and CW-Qbiss panels_AC28
05. The file is ready with basic Qbiss One B, FB, horizontal, Qbiss One B vertical curtain wall.


BIM Library video instructions: 
https://www.youtube.com/@trimodesign/playlists


CONTACT & LINKS
For more information and questions, please contact Trimo technical support on: 
T: 	+386 (0)73 460 200 
M: 	technical@trimo-group.com; 
	trimo@trimo-group.com 

Trimo architectural details:
https://www.trimo-group.com/en/downloads/design-tools/dwg

Trimo BIM libraries: 
www.trimo-group.com/en/downloads/design-tools/bim
 
Trimo technical documents: 
www.trimo-group.com/en/downloads/technical-documents 


DISCLAIMER 
Trimo d.o.o. holds full copyrights on the information and details provided on this media, therefore any unauthorized reproduction and distribution is strictly prohibited. Information/details on this media are for general purposes only. All information issued by Trimo d.o.o. is subject to continuous development and information/details contained on this media are current at the date of issue. It is the user`s responsibility to obtain the most up-to-date information from Trimo when information/details are used for the project. 